For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Were you sent here from the Headlight System Check? | -- | Go to Step 2 | Go to Headlight System Check
2 | Measure the voltage at the head (LH-LWR) fuse. Is the measured voltage equal to the specified value? | B+ | Go to Step 3 | Go to Step 4
3 | Locate and repair the open in the RED/GRN wire between the fuse and the LH headlamp. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Headlight System Check | --
4 | Locate and repair the open in the BLK wire between the fuse and the DIMMER relay. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Headlight System Check | --