For 1990-2009 cars

### Removal Procedure

1. Remove the rear defogger/hazard switch assembly trim plate (1) from the instrument panel (2) by gently prying the 3 clips using a taped flat bladed screwdriver.
2. Disconnect the rear window defogger switch electrical connector (1).
3. Depress the tab on each side of the defogger switch.
4. Remove the rear window defogger switch from the rear defogger/hazard switch assembly trim plate (3).

### Installation Procedure

1. Install the rear window defogger switch to the rear defogger/hazard switch assembly trim plate (3). Ensure that the retaining tabs are fully engaged.
2. Connect the rear window defogger switch electrical connector (1).
3. Press the rear defogger/hazard switch assembly trim plate (3) into the instrument panel. Ensure that the retaining clips are fully engaged.