For 1990-2009 cars

## Side Marker Lamp Bulb Replacement Rear

### Removal Procedure

1. Open the rear compartment lid.
2. Remove the following components from the vehicle:

• | The 4 rear compartment trim panel plastic retainers (2)

• | The rear compartment trim panel (1)

3. Remove the rear side marker bulb socket (2) from the tail lamp.
4. Remove the rear side marker bulb from the bulb socket.

### Installation Procedure

1. Install the rear side marker bulb to the bulb socket.
2. Install the rear side marker bulb socket (2) to the tail lamp.
3. Install the rear compartment trim panel (1) to the vehicle. Secure the trim panel with the 4 plastic retainers (2).
4. Close the rear compartment lid.