For 1990-2009 cars

### Removal Procedure

1. Remove the rear side door lock. Refer to Rear Door Lock Replacement .
2. Remove the following components from the door (2):

• | The 2 bolts (1)

• | The outside door handle (3)

### Installation Procedure

1. Install the outside door handle (3) to the door (2). Secure the handle with the 2 bolts (1).
2. Install the rear side door lock. Refer to Rear Door Lock Replacement .