For 1990-2009 cars

### Removal Procedure

Caution: Always disable the SIR system when servicing the SIR components, or the SIR wiring. Failure to follow the disabling procedures could result in possible deployment, personal injury, or otherwise unneeded SIR system repairs.

1. Disable the SIR system. Refer to Disabling the SIR System .
2. Place the front wheels in the straight ahead position.
3. Remove the steering wheel opening covers (4,8).
4. Remove the bolts (3,9) from the steering wheel module (1).
5. Release the connector position assurance (3) from the inflator module.
6. Disconnect the steering wheel module connector (1).
7. Remove the steering wheel module (2).
8. Fully deploy the module before disposal. If the module was replaced under warranty, fully deploy and dispose of the module after the required retention period. Refer to Inflator Module Handling and Scrapping .

### Installation Procedure

Caution: When you are carrying an undeployed inflator module:

• | Do not carry the inflator module by the wires or connector on the inflator module

• | Make sure the bag opening points away from you

When you are storing an undeployed inflator module, make sure the bag opening points away from the surface on which the inflator module rests. When you are storing a steering column, do not rest the column with the bag opening facing down and the column vertical. Provide free space for the air bag to expand in case of an accidental deployment. Otherwise, personal injury may result.
1. Connect the inflator module electrical connector (1).
2. Connect the connector position assurance (3) to the inflator module.
3. Install the steering wheel module (2).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

4. Install the bolts (3,9) to the steering wheel module.

Tighten
Tighten the bolts to 8.8 N·m (78 lb in).

5. Install the steering wheel opening covers (4,8).
6. Enable the SIR system. Refer to Enabling the SIR System .