For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel (IP) compartment. Refer to Instrument Panel Compartment Replacement in Instrument Panel, Gages and Console.
2. Disconnect the A/C compressor control module electrical connector.
3. Remove the 2 screws and the A/C compressor control module (1).

### Installation procedure

1. Install the A/C compressor control module (1) and secure with the 2 screws.
2. Connect the A/C compressor control module electrical connector.
3. Install the IP compartment. Refer to Instrument Panel Compartment Replacement in Instrument Panel, Gages and Console.