For 1990-2009 cars

(1) | Rear Park Brake Lever Washer
(2) | Rear Brake Shoe Adjuster Actuator
(3) | Rear Park Brake Lever
(4) | Rear Park Brake Lever Retainer Ring
(5) | Rear Park Brake Lever Washer
(6) | Rear Brake Secondary Shoe
(7) | Rear Brake Shoe Holding Spring Cup
(8) | Rear Brake Shoe Holding Spring
(9) | Rear Brake Shoe Holding Spring Cup
(10) | Rear Brake Shoe Return Spring
(11) | Rear Brake Shoe Holding Spring Cup
(12) | Rear Brake Shoe Holding Spring
(13) | Rear Brake Shoe Holding Spring Cup
(14) | Rear Brake Primary Shoe
(15) | Rear Brake Shoe Pin
(16) | Rear Brake Shoe Pin
(17) | Rear Park Brake Lever Strut With The Upper Brake Shoe Return Spring
(18) | Rear Brake Shoe Adjuster Spring

The rear drum brake assembly is a leading/trailing design. When the brakes are applied, the wheel cylinder pistons move both shoes out in order to contact the drum. The shoes contact the drum using enough energy in order to perform the following actions:

• | Overcome the rotation of the wheels

• | Slow the vehicle

• | Stop the vehicle (with continued application).

Adjustment for both the primary and secondary shoes is automatic when the brakes are applied.

Normally, the primary shoe will wear at a faster rate than the secondary shoe. Reinstall the brake shoes in the same position from which the shoes were removed. Do not switch the position of shoes that have been in service. This may render the self-adjustment feature inoperative and result in increased pedal travel.