For 1990-2009 cars

Step | Action | Value(s) | Yes | No
1 | Were you sent here from the Wiper/Washer System Check? | -- | Go to Step 2 | Go to Wiper/Washer System Check
2 |

1. Disconnect the windshield wiper motor connector.
2. Turn the ignition switch to the ON position.
3. Turn the windshield wiper/washer switch to the Off position.
4. Test for B+ at cavity 6 of the windshield wiper motor connector using a J 39200 .

Was the value tested equal to B+?

--

Go to Step 3

Go to Step 6

3 |

1. Disconnect the windshield wiper/washer switch connector.
2. Turn the windshield wiper/washer switch to the off position.
3. Test for continuity between cavity 16 and cavity 7 of the windshield wiper/washer switch using a J 39200 .

Is there continuity between cavity 16 and cavity 7?

--

Go to Step 4

Go to Step 5

4 | Test for continuity between cavity 16 of the windshield wiper/washer switch connector and cavity 5 of the windshield wiper motor connector using a J 39200 . Was there continuity in the BLU/WHT wire? | -- | Go to Step 7 | Go to Step 8
5 | Replace the windshield wiper/washer switch. Refer to Windshield Wiper and Washer Switch Replacement . Is the repair complete? | -- | Go to Wiper/Washer System Check | --
6 | Repair the open in the BLU wire between the windshield wiper motor connector cavity 6 and SP251. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Wiper/Washer System Check | --
7 | Replace the windshield wiper motor. Refer to Windshield Wiper Motor Replacement . Is the repair complete? | -- | Go to Wiper/Washer System Check | --
8 | Repair the open in the BLU/WHT wire between cavity 16 of the windshield wiper/washer switch connector and cavity 5 of the windshield wiper motor connector. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Wiper/Washer System Check | --