For 1990-2009 cars

### Removal Procedure

Important: The automatic transmission control lever solenoid is a part of the brake transmission shift interlock (BTSI) system. The solenoid prevents the operator from shifting the automatic transmission control out of the (P) PARK position, unless the brake pedal is depressed.

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Disconnect the negative battery cable.
2. Remove the front and the rear console assembly. Refer to Console Replacement in Instrument Panel, Gauges, and Console.
3. Disconnect the electrical connector from the shift interlock solenoid (2).
4. Remove the indicator bulb (2).
5. Remove the 2 screws that retain the shift indicator cover (1).
6. Raise and rotate the shift indicator cover to access 2 retaining screws on the shift interlock solenoid.
7. Remove the 2 screws and the shift interlock solenoid.

### Installation Procedure

1. Install the shift interlock solenoid and the 2 screws.
2. Rotate the shift indicator cover (1) back to the original position and firmly snap downward.
3. Install the 2 screws.
4. Connect the electrical connector to the shift interlock solenoid (2).
5. Connect the indicator bulb.
6. Install the rear floor console. Refer to Console Replacement in Instrument Panel, Gauges, and Console.
7. Connect the negative battery cable.