For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Power Windows System Check? | -- | Go to Step 2 | Go to Power Windows System Check
2 |

1. Disconnect the LH window/door lock switch.
2. Connect a fused jumper wire to cavity 4 of the connector
3. Depending on the window's position attach the other end of the jumper wire to one of the following positions:

• | If the window is down cavity 5

• | If the window is up cavity 1

4. Connect a second fused jumper wire to cavity 10 of the connector.
5. Depending on the window's position actuate the other end of the jumper wire to one of the following positions:

• | If the window is down cavity 1

• | If the window is up cavity 5

• | Turn the ignition to the run position.

Did the window move?

--

Go to Step 3

Go to Step 4

3 | Replace the LH window/door lock switch. Refer to Front Side Door Window Switch Replacement . Is the repair complete? | -- | Go to Power Windows System Check | --
4 | Test both the GRN and the YEL wire using a J 39200 DMM between the LH Front window motor and the LH window/door lock switch for an open. Do either of the wires have an open? | -- | Go to Step 5 | Go to Step 6
5 | Repair the open in the wire. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Power Windows System Check | --
6 | Replace the LH front window motor. Refer to Front Side Door Window Regulator Replacement . Is the repair complete? | -- | Go to Power Windows System Check | --