For 1990-2009 cars

### Removal Procedure

1. Disconnect the mass air flow (MAF) sensor.
2. Release the two retaining clips (3).
3. Lift the air cleaner cover (1) up and away from the lower assembly (3).
4. Remove the air cleaner element (2).

### Installation Procedure

1. Install the air cleaner element (2).
2. Lower the air cleaner cover (1) onto the lower assembly (3).
3. Secure the air cleaner cover (2) with the two retaining clips (3).
4. Connect the MAF sensor.