For 1990-2009 cars

### Removal Procedure

1. Remove the dome lamp lens by inserting a flat-bladed tool to the back edge and pushing downward to release the tab.
2. Remove the 2 screws which secure the dome lamp (1).
3. Disconnect the dome lamp electrical connector (1).
4. Remove the dome lamp (2) from the vehicle.
5. Remove the bulb (3) from the dome lamp, if necessary.

### Installation Procedure

1. Install the bulb (3) to the dome lamp (2), if removed.
2. Connect the dome lamp electrical connector (1).
3. Install the dome lamp (1) to the roof. Secure the dome lamp with the 2 screws.
4. Install the dome lamp lens.