For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
1 | Did you perform the Starting System Check? | Go to Step 2 | Go to Starting System Check
2 | Measure the voltage across the battery terminals while cranking the engine. Is the voltage 9.6 volts or more? | Go to Step 3 | Go to Battery Load Test
3 | Measure the voltage between the negative (-) battery terminal and the engine block while cranking the engine. Is the voltage 0-0.5 volts? | Go to Step 5 | Go to Step 4
4 | Replace the negative (-) battery cable. Refer to Battery Cable Replacement . Is the repair complete? | Go to Starting System Check | --
5 | Measure the voltage between the positive (+) battery terminal and the starter solenoid terminal B while cranking the engine. Is the voltage 0-0.5 volts? | Go to Step 6 | Go to Step 7
6 | Repair or replace the starter motor. Refer to Starter Motor Replacement and Starter Motor Overhaul . Is the repair complete? | Go to the Starting System Check | --
7 | Replace the positive (+) battery cable. Refer to Battery Cable Replacement . Is the repair complete? | Go to the Starting System Check | --