For 1990-2009 cars

### Removal Procedure

1. Remove the bolt (2) which secures the windshield washer solvent container (1). Position the washer solvent container in order to gain access to the washer pump.
2. Disconnect the windshield washer pump electrical connector (1).
3. Drain the washer solvent.
4. Remove the windshield washer nozzle hose (3) from the washer pump (2).
5. Remove the washer pump (2) from the washer solvent container (1).

### Installation Procedure

1. Install the windshield washer pump (2) to the windshield washer solvent container (1).
2. Install the windshield washer nozzle hose (3) to the washer pump (2).
3. Connect the washer pump electrical connector (1).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

4. Install the washer solvent container (1) to the vehicle. Secure the container with the bolt (2).

Tighten
Tighten the washer solvent container bolt to 5.5 N·m (49 lb in).

5. Fill the washer solvent container (1) with washer solvent.