For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Exhaust Manifold Pipe Drive Shaft Heat Shield Bolt | 5.4 N·m | 48 lb in
Exhaust Manifold Pipe Drive Shaft Heat Shield Nut | 5.4 N·m | 48 lb in
Exhaust Pipe to Exhaust Manifold Bolt | 62 N·m | 46 lb ft
Front Suspension Brace Nut | 69 N·m | 51 lb ft
Inner Tie Rod-to-Steering Rack | 62 N·m | 46 lb ft
Lower Engine Splash Shield Bolt | 10 N·m | 89 lb in
Outer Tie Rod-to-Inner Tie Rod Jam Nut | 56 N·m | 41 lb ft
Power Steering Fluid Reservoir Bracket Bolt | 5.4 N·m | 48 lb in
Power Steering Fluid Reservoir Inlet Pipe/Hose Clip Bolt | 5.4 N·m | 48 lb in
Power Steering Gear Boot Heat Shield Bolt | 5.4 N·m | 48 lb in
Power Steering Gear Boot Heat Shield Nut | 10 N·m | 89 lb in
Power Steering Gear Clamp Bolt | 71 N·m | 52 lb ft
Power Steering Gear Clamp Nut | 71 N·m | 52 lb ft
Power Steering Gear Inlet Hose Fitting | 54 N·m | 40 lb ft
Power Steering Gear Inlet Pipe Clip Bolt | 5.4 N·m | 48 lb in
Power Steering Gear Inlet Pipe Nut | 13 N·m | 9 lb ft
Power Steering Gear Outlet Front Pipe Nut | 13 N·m | 9 lb ft
Power Steering Gear Outlet Pipe Clip Bolt | 5.4 N·m | 48 lb in
Power Steering Gear Outlet Pipe Heat Shield Bolt | 5.4 N·m | 48 lb in
Power Steering Pressure Switch | 21 N·m | 15 lb ft
Power Steering Pulley Nut | 43 N·m | 32 lb ft
Power Steering Pump Nut | 37 N·m | 27 lb ft
Rear Transaxle Mount Bracket Bolt | 77 N·m | 57 lb ft
Rear Transaxle Mount Through Bolt | 87 N·m | 64 lb ft
Return Elbow Flare Nut | 44 N·m | 32 lb ft
Steering Column Upper Cover Bolt | 4.9 N·m | 43 lb in
Steering Shaft Lower Coupling Bolt | 35 N·m | 26 lb ft