For 1990-2009 cars

### Removal Procedure

1. Open the rear compartment lid.
2. Remove the following components from the vehicle:

• | The 4 rear compartment trim panel plastic retainers (2)

• | The rear compartment trim panel (1)

3. Remove the turn signal lamp socket (1) from the tail lamp.
4. Remove the turn signal lamp bulb from the lamp socket (1).

### Installation Procedure

1. Install the turn signal lamp bulb to the lamp socket (1).
2. Install the turn signal lamp socket (1) to the tail lamp.
3. Install the rear compartment trim panel (1) to the vehicle. Secure the trim panel with the 4 plastic retainers (2).
4. Close the rear compartment lid.