For 1990-2009 cars

### Outside Rearview Mirror

Battery voltage is supplied to terminal 9 of the outside rearview mirror switch when the ignition switch is in the ON or ACC position. Ground is supplied to terminal 10 of the outside rearview mirror switch at all times. Battery voltage and ground are supplied to the left and right outside rear view mirror motors through 6 wires located in the following terminals of the outside rearview mirror switch:

• | Terminal 1

• | Terminal 5

• | Terminal 6

• | Terminal 7

• | Terminal 8