For 1990-2009 cars

### Removal Procedure

1. Remove the radio. Refer to Radio Replacement Radio Replacement in Entertainment.
2. Remove the instrument panel compartment. Refer to Instrument Panel Compartment Replacement .
3. Remove the I/P drivers knee bolster reinforcement. Refer to Knee Bolster Replacement .
4. Remove the front floor rear console. Refer to Console Replacement .
5. Remove the manual transaxle control lever boot, if equipped. Refer to Console Shift Boot Replacement .
6. Remove the automatic transaxle control opening cover bezel, if equipped. Refer to Console Trim Plate Replacement .
7. Remove the 2 screws which secure the front floor front console (2) to the instrument panel assembly.
8. Pull the front floor console (2) rearward and up.
9. Remove the front floor console (2) from the vehicle.

### Installation Procedure

1. Install the front floor front console (2) to the vehicle. Secure the console to the instrument panel with the 2 screws.
2. Install the front floor rear console. Refer to Console Replacement .
3. Install the automatic transaxle control opening cover bezel (1), if equipped. Refer to Console Trim Plate Replacement .
4. Install the manual transaxle control lever boot, if equipped. Refer to Console Shift Boot Replacement .
5. Install the I/P drivers knee bolster reinforcement. Refer to Knee Bolster Replacement .
6. Install the instrument panel compartment. Refer to Instrument Panel Compartment Replacement .
7. Install the radio. Refer to Radio Replacement Radio Replacement in Entertainment.