For 1990-2009 cars

#### Tools Required

J 9617 Oil Pump Seal Installer

### Removal Procedure

1. Remove the oil seal from the pump.
2. Inspect the seal contact portion of the torque converter.

Clean the seal contact portion of the torque converter.

### Installation Procedure

1. Install the oil seal.
2. Apply GM P/N 1050169 grease to the oil seal lip.
3. Use the J 9617 to drive in the oil seal.