For 1990-2009 cars

Notice: Use of harsh chemicals when cleaning can damage exterior lamps. Suggested cleaners are a mild soap and water, or Varnish Makers and Painters (VM&P) Naptha. VM&P Naptha is a specific type of naptha and should not be substituted by any other naptha.

1. Wash the affected area with soap and water.
2. Wipe the area dry.
3. Wipe the panel and the adhesive side of the molding with a clean rag using oil-free naphtha or alcohol.
4. Do NOT remove the tape from the body if the molding has pulled loose from the adhesive backing.
5. Clean the back of the molding and the tape on the body using oil-free naphtha or alcohol.
6. Apply masking tape (1) or use a straightedge as a molding guide in order to ensure that the molding is straight.
7. Apply Goodwrench trim body adhesive GM P/N 12345632 (Canadian P/N 10953475) or equivalent to the back of the molding.
8. Press the molding into place.
9. Apply constant pressure to the molding for 30 seconds or until a firm bond is made.