For 1990-2009 cars

### Removal Procedure

1. Using a taped flat bladed tool, gently pry and release the 4 clips around the lamp dimmer switch/remote control rearview mirror switch trim plate (2).
2. Disconnect the outside remote control rearview mirror switch electrical connector (1).
3. Remove the outside remote control rearview mirror switch from the trim plate by depressing the 4 retaining tabs.

### Installation Procedure

1. Install the outside remote control rearview mirror switch to the lamp dimmer switch/remote control rearview mirror switch trim plate (3). Ensure that the retaining tabs are fully engaged.
2. Connect the outside remote control rearview mirror switch electrical connector (1).
3. Install the lamp dimmer switch/remote control rearview mirror switch trim plate (3) to the I/P. Ensure that the retaining clips are fully engaged.