For 1990-2009 cars

### Removal Procedure

1. Remove the front seat cushion. Refer to Front Seat Cushion Replacement .
2. Remove the head restraint (1) from the seat back cushion (3).
3. Gently pry the head restraint guides (1) from the seat back cushion (2) using a flat bladed tool.
4. Cut and remove the hog rings (2).
5. Roll the seat back cushion cover (1) upward slowly and evenly.
6. Remove the seat back cushion pad from the frame, if necessary.

### Installation Procedure

1. Install the seat back cushion pad to the frame, if removed.
2. Roll the seat back cushion cover (1) down over the seat back cushion.
3. Use hog ring pliers to install new hog rings (2). Ensure that the seat back cushion cover is secure.
4. Install the head restraint guides (2) to the seat back cushion (3).
5. Install the head restraint (1) to the seat back cushion (3).
6. Install the front seat cushion. Refer to Front Seat Cushion Replacement .