For 1990-2009 cars

#### Tools Required

J-38125 Terminal Repair Kit

### Removal Procedure

1. Remove the steering wheel inflatable restraint module. Refer to Inflatable Restraint Steering Wheel Module Replacement in SIR.
2. Disconnect the cruise control switch electrical connector (1) from the steering wheel inflatable restraint module coil.
3. Open the Terminal Position Assurance (TPA) on the top of the cruise control switch electrical connector with a terminal remover from the J-38125 .
4. Remove the red/blue wire (2) from the cruise control switch electrical connector (1) with a terminal remover from the J-38125 .
5. Using a allen head socket, remove the right horn contact bolts.
6. Remove the right horn contact (2) from the steering wheel.
7. Remove the following components from the vehicle:

• | The 3 cruise control switch screws (4)

• | The cruise control switch (3)

### Installation Procedure

1. Install the cruise control switch (3) to the vehicle. Secure the switch with the 3 screws (4).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the right horn contact (2) to the steering wheel. Secure the contact with the 2 allen head bolts.

Tighten
Tighten the horn contact bolts to 8.8 N·m (78 lb in).

3. Install the red/blue wire (2) to the cruise control switch electrical connector (1).
4. Close the TPA on the top of the cruise control switch electrical connector.
5. Connect the cruise control switch electrical connector (1) to the steering wheel inflatable restraint module coil.
6. Install the steering wheel inflatable restraint module. Refer to Inflatable Restraint Steering Wheel Module Replacement in SIR.