For 1990-2009 cars

### Removal Procedure

1. Remove the fuel sender assembly. Refer to Fuel Sender Assembly Replacement .
2. Remove the end cap (1) and the lower cushion from the fuel sender assembly .
3. Remove the fuel pressure regulator.
4. Remove the retaining clip (1) from the fuel pump strainer .
5. Remove the fuel pump strainer (2).
6. Remove the fuel sender assembly housing (2) from the fuel level sensor and gauge unit assembly (1).
7. Remove the fuel filter cushion from the fuel filter.
8. Disconnect the electrical connector (4) from the fuel pump .
9. Remove the fuel pump (3) from the fuel filter (2).
10. Remove the fuel filter (2) from the fuel level sensor and gauge unit assembly (1).

### Installation Procedure

1. Install the fuel filter (2) to the fuel level sensor and gauge unit assembly (1).
2. Install the fuel pump (3) into the fuel filter (2).
3. Connect the electrical connector (4) to the fuel pump .
4. Install the fuel filter cushion to the fuel filter (2) .
5. Install the fuel sender assembly housing (3) to the fuel level sensor and gauge unit assembly (1).
6. Install the fuel pressure regulator (4) to the bottom of the fuel filter (2).
7. Install the fuel pump strainer (2) to the fuel pump.
8. Secure the strainer with the clip (1).
9. Install the lower cushion to the bottom of the fuel pump.
10. Install the fuel sender assembly end cap (1).
11. Install the fuel sender assembly into the fuel tank. Refer to Fuel Sender Assembly Replacement .