For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Power Windows System Check? | -- | Go to Step 2 | Go to Power Windows System Check
2 |

1. Disconnect the RH front window switch.
2. Turn the ignition switch to the RUN position.
3. Using a test lamp, probe cavity 4 of the connector.

Does the test lamp illuminate?

--

Go to Step 3

Go to Step 4

3 |

1. Turn the ignition switch to the OFF position.
2. Disconnect the LH window/door lock switch connector.
3. Test for an open in the wire using a J 39200 DMM from cavity 2 of the RH front door connector to the cavity 6 of the LH front door connector.

Does the wire have an open?

--

Go to Step 6

Go to Step 5

4 | Repair the open in the BLK wire from the connector or replace SP252, as needed. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Power Windows System Check | --
5 | Test for an open in the GRN/RED wire using a J 39200 DMM from cavity 5 of the RH front door connector to cavity 14 of the LH window/door connector. Does the wire have an open? | -- | Go to Step 7 | Go to Step 8
6 | Repair the open in the BLU/WHT wire between the right and left door switches. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Power Windows System Check | --
7 | Repair the open in the GRN/RED wire between the left and right door switches. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Power Windows System Check | --
8 |

1. Reconnect the left door connector.
2. Turn the ignition to the Run position.
3. Using a test lamp, probe cavity 2 of the right door connector to ground and activate the left door switch to the window DOWN position.
4. Using a test lamp, probe cavity 5 of the right door connector to ground and activate the left door switch to the window UP position.

Does the test lamp illuminate in each case?

--

Go to Step 9

Go to Step 10

9 |

1. Reconnect the right door connector.
2. Using a test lamp, backprobe cavity 1 of the right door connector to ground and activate the right door switch to the DOWN position.
3. Using a test lamp, backprobe cavity 3 of the right door connector to ground and activate the right door switch to the UP position.

Does the test lamp illuminate in each case?

--

Go to Step 11

Go to Step 12

10 | Replace the LH window/door lock switch. Refer to Front Side Door Window Switch Replacement . Is the repair complete? | -- | Go to Power Windows System Check | --
11 | Test for an open in the GRN wire using a J 39200 DMM between the switch connector cavity 1 and the motor connector cavity 1. Does the wire have an open? | -- | Go to Step 14 | Go to Step 13
12 | Replace the RH front window switch. Refer to Front Side Door Window Switch Replacement . Is the repair complete? | -- | Go to Power Windows System Check | --
13 | Test for an open in the YEL wire using a J 39200 DMM between the switch connector cavity 1 and the motor connector cavity 1. Does the wire have an open? | -- | Go to Step 16 | Go to Step 15
14 | Repair the open in the GRN wire between the switch and the motor. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Power Windows System Check | --
15 | Replace the motor. Refer to Front Side Door Window Regulator Replacement . Is the repair complete? | -- | Go to Power Windows System Check | --
16 | Repair the open in the YEL wire between the switch and the motor. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Power Windows System Check | --