For 1990-2009 cars

### Removal Procedure

1. Unclip and remove the inner mirror garnish (2) from the door.
2. Remove the following components from the door:

• | The 3 nuts

• | The outside rearview mirror (1)

### Installation Procedure

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Install the outside rearview mirror (1) to the door. Secure the mirror with the 3 nuts.

Tighten
Tighten the outside rearview mirror nuts to 15 N·m (11 lb ft).

2. Install the inner mirror garnish (2) to the door.