For 1990-2009 cars

### Removal Procedure

1. Open the hood.
2. Disconnect the backup lamp switch electrical connector (2).
3. Remove the backup lamp switch (1) from the transaxle case.

### Installation Procedure

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

Important: The backup lamp switch should have pre-applied thread sealant on the threads.

1. Install the backup lamp switch (1) to the transaxle case.

Tighten
Tighten the backup lamp switch to 20 N·m (15 lb ft).

2. Connect the backup lamp switch electrical connector (2).
3. Close the hood.