For 1990-2009 cars

### Removal Procedure

1. Unclip and remove the trim cover (2) from the front side door armrest.
2. Remove the 2 screws (2) that retain the front side door trim panel (1).
3. Remove the front side door window regulator handle by using a cloth in order to pull off the snap ring, if equipped.
4. Using a taped flat bladed tool, gently pry the front side door accessory switch mounting plate (1) from the front side door trim (2), if equipped.
5. Disconnect the front side door window and/or lock switch electrical connectors (2, 3), if equipped.
6. Remove the front side door accessory switch mounting plate (1) from the vehicle, if equipped.
7. Remove the plastic retainer (3) that retains the front side door trim (1).
8. Remove the front side door inside handle. Refer to Front Side Door Inside Handle Replacement .
9. Remove the front side door trim (1) from the door by disengaging the plastic retainers.

### Installation Procedure

1. Position and install the front side door trim (1) to the door and press the plastic retainers into place. Ensure that the plastic retainers are completely engaged. Secure the door trim with the plastic retainer (3).
2. Install the front side door inside handle. Refer to Front Side Door Inside Handle Replacement .
3. Connect the front side door window and/or lock switch electrical connectors (2, 3), if equipped.
4. Install the front side door accessory switch mounting plate (1) to the front side door trim, if equipped.
5. Install the front side door window regulator handle snap ring (1) to the front side door window regulator handle (2), if equipped.
6. Install the regulator handle (2) to the door, if equipped.
7. Install the 2 screws (2) that retain the front side door trim panel (1).
8. Install the trim cover to the front side door armrest.