For 1990-2009 cars
ABS Components
Antilock Brake System Schematics
Handling ESD Sensitive Parts Notice

### Circuit Description

The right rear solenoid valve is part of Brake Pressure Modulator Valve (BPMV). The BPMV turns ON and OFF the right rear solenoid valve as deemed necessary to modulate brake hydraulic pressure to the right rear wheel brake during an ABS stop.

### Conditions for Running the DTC

DTC 0060 can be set anytime the ignition switch is in the ON position.

### Conditions for Setting the DTC

The Electronic Brake Control Module (EBCM) detects any of the following in the right rear solenoid circuitry:

• | an open

• | short to ground

• | a short to voltage

### Action Taken When the DTC Sets

• | The ABS disables

• | The ABS warning indicator turns ON

### Conditions for Clearing the DTC

The condition responsible for setting the DTC no longer exists and the Scan Tool Clear DTCs function is used.

### Diagnostic Aids

If DTC C0125 (Value Relay Circuit Open) is set (current or history) go to the DTC C0125 table first.

### Test Description

The numbers below refer to step numbers on the Diagnostic Table.

1. This step determines whether the DTC is current.

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform A Diagnostic System Check - ABS? | -- | Go to Step 2 | Go to Diagnostic System Check - ABS
2 |

1. Install a scan tool.
2. Turn ON the ignition, with the engine OFF.
3. Use the scan tool in order to clear the DTCs.
4. Using the scan tool, cycle the appropriate solenoid in the Special Functions menu.
5. Read the DTCs.

Does the DTC reset?

--

Go to Step 3

Go to Testing for Intermittent Conditions and Poor Connections in Wiring Systems

3 |

1. Test the Solenoid Input circuit for an open, high resistance, or a short to ground. Refer to Circuit Testing and Wiring Repairs in Wiring Systems.
2. Test the Solenoid Ground circuit for an open or high resistance. Refer to Circuit Testing and Wiring Repairs in Wiring Systems.

Was a problem found and corrected?

--

Go to Diagnostic System Check - ABS

Go to Step 4

4 | Replace the Brake Modulator Assembly. Refer to Brake Pressure Modulator Valve Assembly Replacement . Is the repair complete? | -- | Go to Step 5 | --
5 |

1. Use the scan tool in order to clear the DTCs.
2. Using the scan tool, cycle the appropriate solenoid in the Special Functions menu.
3. Read the DTCs.

Does the DTC reset?

--

Go to Step 2

System OK