For 1990-2009 cars

### Removal Procedure

1. Remove the left and right rear end trim finish panels. Refer to Rear Compartment Side Trim Replacement - Left Side and Rear Compartment Side Trim Replacement - Right Side .
2. Remove the following components from the vehicle:

• | The 2 plastic retainers

• | The rear compartment sill trim plate (1)

### Installation Procedure

1. Install the rear compartment sill trim plate (1) to the vehicle. Secure the trim plate with the 2 plastic retainers.
2. Install the left and right rear end trim finish panels. Refer to Rear Compartment Side Trim Replacement - Left Side and Rear Compartment Side Trim Replacement - Right Side .