For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Counter Driven Gear Nut | 172.0 N·m | 127.0 lb ft
Detent Spring | 10.0 N·m | 89.0 lb in
Differential Carrier Cover Bolts | 25.0 N·m | 18.0 lb ft
Differential Ring Gear Bolts | 97.0 N·m | 71.0 lb ft
Left Bearing Retainer Bolts | 19.0 N·m | 14.0 lb ft
Manual Valve and Body Bolts | 10.0 N·m | 89.0 lb in
Oil Pan Bolts | 5.0 N·m | 44.0 lb in
Oil Pipe Nuts | 34.0 N·m | 25.0 lb ft
Oil Pump-to-Case Bolts | 22.0 N·m | 16.0 lb ft
Oil Pump Body Bolts | 10.0 N·m | 89.0 lb in
Oil Strainer Bolts | 10.0 N·m | 89.0 lb in
Oil Tube Bracket Bolt | 10.0 N·m | 89.0 lb in
Park/Neutral Position (PNP) Switch Lever Nut | 7.0 N·m | 62.0 lb in
Park/Neutral Position (PNP) Switch Mounting Bolts | 5.5 N·m | 49.0 lb in
Right Union Bearing Cap Bolts | 49.0 N·m | 36.0 lb ft
Torque Converter-to-Drive Plate Bolts | 64.0 N·m | 47.0 lb ft
Transaxle Rear Cover Bolts | 25.0 N·m | 18.0 lb ft
Valve Body-to-Case Bolts | 10.0 N·m | 89.0 lb in
Valve Body Upper and Lower Bolts | 5.5 N·m | 49.0 lb in

Application | Specification
--- | ---
Metric | English
Accumulator Cover Bolts | 10 N·m | 89 lb in
Air Cleaner (ACL) Bolts | 12 N·m | 106 lb in
Apply Pipe Bracket Bolts | 10 N·m | 89 lb in
Center Crossmember Rear Bolt and Nuts | 61 N·m | 45 lb ft
Detent Spring Bolts | 10 N·m | 89 lb in
Differential Drain Plug | 39 N·m | 29 lb ft
Differential Filler Plug | 39 N·m | 29 lb ft
Fluid Cooler Inlet Pipe Bracket Bolt | 5 N·m | 44 lb in
Fluid Cooler Outlet Pipe Bracket Bolt | 5 N·m | 44 lb in
Fluid Filler Tube Bracket Bolt | 5 N·m | 44 lb in
Fluid Filter Screen Bolts | 10 N·m | 89 lb in
Flywheel-to-Torque Converter Bolts | 19 N·m | 14 lb ft
Front Exhaust Pipe Support Bolts | 19 N·m | 14 lb ft
Front Exhaust Pipe Support Nuts and Bolts | 19 N·m | 14 lb ft
Front Exhaust Pipe-to-Ehaust Manifold Nuts | 62 N·m | 46 lb ft
Front Exhaust Pipe-to-TWC Mating Flange Bolts | 43 N·m | 32 lb ft
Front Suspension Crossmember Bolts | 206 N·m | 152 lb ft
Front Transaxle Mount Bolts | 64 N·m | 47 lb ft
Front Transaxle Mount Through Bolt and Nut | 87 N·m | 64 lb ft
Governor Cover Retaining Bolts | 13 N·m | 115 lb in
Ground Strap Bolt | 13 N·m | 115 lb in
Inlet and Outlet Fluid Cooler Pipe Flare Nuts | 27 N·m | 20 lb ft
Inner Shift Select Cable Grommet Retainer Bolts | 5 N·m | 44 lb in
Left Drive Axle Stone Shield Bolts | 5 N·m | 44 lb in
Left Transaxle Mount Through Bolt | 87 N·m | 64 lb ft
Left Transaxle Mounting Bracket Bolts | 56 N·m | 41 lb ft
Left Transaxle Mounting Bracket Reinforcement Bolts | 21 N·m | 15 lb ft
Lower Engine Reinforcement Brace Bolts | 64 N·m | 47 lb ft
Lower Valve Body Bolts | 5.4 N·m | 48 lb in
Manual Lever Nut | 12 N·m | 106 lb in
Manual Selector Bolts | 13 N·m | 115 lb in
Manual Shaft Nut | 6.9 N·m | 61 lb in
Manual Valve Body Bolts | 10 N·m | 89 lb in
Outer Shift Select Cable Grommet Retainer Bolts | 5 N·m | 44 lb in
Outlet Fluid Cooler Pipe Flare Nuts | 27 N·m | 20 lb ft
Park/Neutral Position (PNP) Switch Bolts | 5.4 N·m | 48 lb in
Rear Transaxle Mount Nuts | 57 N·m | 42 lb ft
Rear Transaxle Mount Through Bolt | 87 N·m | 64 lb ft
Right Kick Panel Plastic Nut | 5.4 N·m | 48 lb in
Shift Select Cable Nut | 12 N·m | 106 lb in
Solenoid Wire Harness Retaining Bolt | 6 N·m | 53 lb in
Splash Shield Bolts | 5 N·m | 44 lb in
Throttle Valve Cam Bolt | 10 N·m | 89 lb in
Transaxle Cooler Pipe Retaining Bracket Bolt | 10 N·m | 7.5 lb in
Transaxle Drain Plug | 23 N·m | 17 lb ft
Transaxle Fluid Pan Bolts | 4.9 N·m | 43 lb in
Transaxle-to-Engine Bolts | 64 N·m | 47 lb ft
TV Cable Adjust Nut | 8 N·m | 71 lb in
TV Cable Guide Bracket Bolt | 8 N·m | 71 lb in
TV Cable Locknut | 8 N·m | 71 lb in
TV Cable Retaining Bolt | 8 N·m | 71 lb in
Upper Valve Body Bolts | 5.4 N·m | 48 lb in
Valve Body Assembly Bolts | 10 N·m | 89 lb in
Vehicle Speed Sensor (VSS) Bolt | 6 N·m | 53 lb in