For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Were you sent here from the Interior Lights System Check? | -- | Go to Step 2 | Go to Interior Lamps System Check
2 | Disconnect the rear compartment lamp switch connector. Is the rear compartment lamp OFF? | -- | Go to Step 4 | Go to Step 3
3 | Repair the short to ground in the RED/WHT wire from the rear compartment lamp cavity 2. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Interior Lamps System Check | --
4 | Replace the rear compartment lamp switch. Refer to Rear Compartment Lid Switch Replacement in Body Rear End. Is the repair complete? | -- | Go to Interior Lamps System Check | --