For 1990-2009 cars

#### Interior Lights System Check

Step | Action | Normal Result(s) | Abnormal Result(s)*
--- | --- | --- | ---
1 | Turn the Sunroof Map Lamp switch to the ON position. | The Map Lamp illuminates. | Courtesy/Reading Lamps Inoperative
2 | Turn the Sunroof Map Lamp switch to the OFF position. | The Map Lamp extinguishes. | Courtesy Lamps Always On .
3 | Perform any of the following:

• | Turn the Dome Lamp switch to the ON position.

• | Activate the keyless entry to unlock the doors.

• | Open any door.

The Dome Lamp will illuminate.

Courtesy or Dome Lamps Inoperative

4 | Turn the Dome Lamp switch to the OFF position with the doors CLOSED. | The Dome Lamp does not illuminate. | Dome Lamps Always On
5 | Open the trunk. | The Rear Compartment Lamp Illuminates. | Rear Compartment Lamp Inoperative
6 | Close the trunk. | The Rear Compartment Lamp extinguishes. | Rear Compartment Lamp Always On
* Refer to the appropriate symptom diagnostic table for the applicable abnormal result.