For 1990-2009 cars

## Door Lock Rod Knob Replacement Front

### Removal Procedure

1. Remove the front side door trim. Refer to Front Side Door Trim Panel Replacement .
2. Remove the lock rod knob (5) from the front door locking rod by unscrewing in a counterclockwise direction.

### Installation Procedure

1. Install the lock rod knob (5) to the front door locking rod by turning in a clockwise direction.
2. Install the front side door trim. Refer to Front Side Door Trim Panel Replacement .

## Door Lock Rod Knob Replacement Rear

### Removal Procedure

1. Remove the rear side door trim. Refer to Rear Side Door Trim Panel Replacement .
2. Remove the lock rod knob (3) from the rear door locking rod by unscrewing in a counterclockwise direction.

### Installation Procedure

1. Install the lock rod knob (3) to the rear door locking rod by turning in a clockwise direction.
2. Install the rear side door trim. Refer to Rear Side Door Trim Panel Replacement .