For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel compartment. Refer to Instrument Panel Compartment Replacement in Instrument Panel, Gages and Console.
2. Disconnect the cruise control module electrical connector.
3. Remove the following components from the vehicle:

• | The cruise control module mounting bolt

• | The cruise control module (2)

### Installation Procedure

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Install the cruise control module (2) to the IP. Secure the module with the mounting bolt.

Tighten
Tighten the cruise control module mounting bolt to 10 N·m (89 lb in).

2. Connect the cruise control module electrical connector.
3. Install the instrument panel compartment. Refer to Instrument Panel Compartment Replacement in Instrument Panel, Gages and Console.