For 1990-2009 cars

Application | Specifications
--- | ---
Metric | English
Countershaft Driven Gear Locknut | 177 N·m | 131 lb ft
Countershaft Front Roller Bearing Retaining Bolt | 17 N·m | 13 lb ft
Differential Ring Gear Bolts | 97 N·m | 72 lb ft
Fluid Cooler Pipe Bracket Bolt | 5 N·m | 44 lb in
Fluid Cooler Pipe Unions | 29 N·m | 21 lb ft
Fluid Filler Tube Bracket Bolt | 5 N·m | 44 lb in
Fluid Filter Screen Bolts | 10 N·m | 89 lb in
Fluid Pipe Clamp Bolts | 5 N·m | 44 lb in
Fluid Pump Bolts | 25 N·m | 18 lb ft
Front Fluid Baffle Bolt | 10 N·m | 89 lb in
Front Transaxle Mounting Bracket Bolts | 23 N·m | 17 lb ft
Gallery Cover Bolts | 10 N·m | 89 lb in
Gallery Cover TORX® Head Screws | 7 N·m | 62 lb in
Inlet and Outlet Fluid Cooler Pipe Fittings | 34 N·m | 25 lb ft
Intermediate Shaft Locknut | 177 N·m | 131 lb ft
Left Transaxle Mounting Bracket Bolts | 23 N·m | 17 lb ft
Lower-to-Upper Valve Body Bolt A, 50 mm (1.97 in) | 6 N·m | 53 lb in
Lower-to-Upper Valve Body Bolt B, 38 mm (1.5 in) | 6 N·m | 53 lb in
Lower-to-Upper Valve Body Bolt C, 20 mm (0.79 in) | 10 N·m | 89 lb in
Manual Detent Spring Bolt | 10 N·m | 89 lb in
Manual Lever Nut | 13 N·m | 115 lb in
Manual Shaft Nut | 12 N·m | 106 lb in
Parking Lock Guide Bolts | 13 N·m | 115 lb in
Parking Pawl Shaft Retaining Bolt | 5 N·m | 44 lb in
Park/Neutral Position (PNP) Switch Bolts | 5 N·m | 44 lb in
Pressure Relief Valve Retaining Bolts | 6 N·m | 53 lb in
Rear Case Cover Bolts | 10 N·m | 89 lb in
Rear Fluid Baffle Bolt | 10 N·m | 89 lb in
Rear Transaxle Mounting Bracket Bolts | 23 N·m | 17 lb ft
Shift Select Cable Bracket Bolts | 5 N·m | 44 lb in
Solenoid Retaining Bolts | 6 N·m | 53 lb in
Solenoid Wire Harness Clip Bolt | 6 N·m | 53 lb in
Solenoid Wire Harness Retaining Bolt | 5 N·m | 44 lb in
Stator Shaft-to-Fluid Pump Body Bolts | 10 N·m | 89 lb in
Throttle Valve Cam Bolt | 10 N·m | 89 lb in
Torque Converter Housing Bolts | 29 N·m | 21 lb ft
Transaxle Fluid Pan Bolts | 5 N·m | 44 lb in
Transaxle Holding Fixture Bolts | 11 N·m | 98 lb in
TV Cable Retaining Bolt | 5 N·m | 44 lb in
Valve Body Assembly Bolts | 10 N·m | 89 lb in
2nd Coast Brake Band Guide Bolt | 10 N·m | 89 lb in
2nd Coast Brake Servo Apply Pipe Bracket Bolt | 5 N·m | 44 lb in

Application | Specification
--- | ---
Metric | English
Air Cleaner (ACL) Bolts | 12 N·m | 106 lb in
Center Crossmember Rear Bolt and Nuts | 61 N·m | 45 lb ft
Detent Spring Bolts | 10 N·m | 89 lb in
Fluid Cooler Inlet Pipe Bracket Bolt | 5 N·m | 44 lb in
Fluid Cooler Outlet Pipe Bracket Bolt | 5 N·m | 44 lb in
Fluid Filler Tube Bracket Bolt | 5 N·m | 44 lb in
Fluid Filter Screen Bolts | 10 N·m | 89 lb in
Flywheel-to-Torque Converter Bolts | 19 N·m | 14 lb ft
Front Exhaust Pipe Support Bolts | 19 N·m | 14 lb ft
Front Exhaust Pipe Support Nuts and Bolts | 19 N·m | 14 lb ft
Front Exhaust Pipe-to-Exhaust Manifold Nuts | 62 N·m | 46 lb ft
Front Exhaust Pipe-to-TWC Mating Flange Bolts | 43 N·m | 32 lb ft
Front Suspension Crossmember Bolts | 206 N·m | 152 lb ft
Front Transaxle Mount Bolts | 64 N·m | 47 lb ft
Front Transaxle Mount Through Bolt and Nut | 87 N·m | 64 lb ft
Ground Strap Bolt | 34 N·m | 25 lb ft
Inlet and Outlet Fluid Cooler Pipe Flare Nuts | 27 N·m | 20 lb ft
Inner Shift Select Cable Grommet Retainer Bolts | 5 N·m | 44 lb in
Left Drive Axle Stone Shield Bolts | 5 N·m | 44 lb in
Left Transaxle Mount Through Bolt | 87 N·m | 64 lb ft
Left Transaxle Mounting Bracket Bolts | 56 N·m | 41 lb ft
Left Transaxle Mounting Bracket Reinforcement Bolts | 21 N·m | 15 lb ft
Lower Engine Reinforcement Brace Bolts | 64 N·m | 47 lb ft
Lower Valve Body-to-Upper Valve Body Bolts 38 mm (1.50 in) | 6.4 N·m | 57 lb in
Lower Valve Body-to-Upper Valve Body Bolts 25 mm (0.98 in) | 10 N·m | 89 lb in
Manual Lever Nut | 12 N·m | 106 lb in
Manual Selector Bolts | 13 N·m | 115 lb in
Manual Shaft Nut | 6.9 N·m | 61 lb in
Outer Shift Select Cable Grommet Retainer Bolts | 5 N·m | 44 lb in
Pressure Relief Valve Retaining Bolt | 6.4 N·m | 57 lb in
Park/Neutral Position (PNP) Switch Bolts | 5.4 N·m | 48 lb in
Rear Transaxle Mount Nuts | 57 N·m | 42 lb ft
Rear Transaxle Mount Through Bolt | 87 N·m | 64 lb ft
Right Kick Panel Plastic Nut | 5.4 N·m | 48 lb in
Shift Select Cable Nut | 12 N·m | 106 lb in
Shift Solenoid Retaining Bolt | 6.4 N·m | 57 lb in
Solenoid Wire Harness Clip Bolt | 6 N·m | 53 lb in
Solenoid Wire Harness Retaining Bolt | 6 N·m | 53 lb in
Solenoid Wiring Harness Retaining Bracket Bolt | 20 N·m | 15 lb ft
Splash Shield Bolts | 5 N·m | 44 lb in
Throttle Valve Cam Bolt | 10 N·m | 89 lb in
Torque Converter Clutch (TCC) Solenoid Retaining Bolt | 6.4 N·m | 57 lb in
Transaxle Drain Plug | 17 N·m | 13 lb ft
Transaxle Cooler Pipe Retaining Bracket Bolt | 10 N·m | 7.5 lb in
Transaxle Drain Plug | 23 N·m | 17 lb ft
Transaxle Fluid Pan Bolts | 4.9 N·m | 43 lb in
Transaxle Solenoid Wire Harness Retaining Bolt | 5.5 N·m | 49 lb in
Transaxle-to-Engine Bolts | 64 N·m | 47 lb ft
TV Cable Adjust Nut | 8 N·m | 71 lb in
TV Cable Guide Bracket Bolt | 8 N·m | 71 lb in
TV Cable Locknut | 8 N·m | 71 lb in
TV Cable Retaining Bolt | 8 N·m | 71 lb in
Valve Body Assembly Bolts | 10 N·m | 89 lb in
Vehicle Speed Sensor (VSS) Bolt | 6 N·m | 53 lb in