For 1990-2009 cars

### Removal Procedure

1. Remove the instrument cluster retainer. Refer to Instrument Panel Cluster Trim Plate Bezel Replacement .

Important: Do not remove the needle from the temperature gauge. There is no detent or flat spot on the shaft in order to indicate the correct placement.

2. Remove the 3 screws (4) which secure the temperature gauge to the instrument cluster case.
3. Remove the temperature gauge (4) from the instrument cluster case.

### Installation Procedure

1. Install the temperature gauge (4) to the instrument cluster case.
2. Secure the temperature gauge with the 3 screws (4).
3. Install the instrument cluster retainer. Refer to Instrument Panel Cluster Trim Plate Bezel Replacement .