For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
1 |

1. Use a known functional transmitter in order to program the system.
2. Retest the keyless entry system.

Does the system respond properly?

Go to Step 2

Go to Step 3

2 |

1. Replace the inoperative transmitter.
2. Reprogram the RKE module. Refer to Transmitter Programming .

Is the replacement complete?

System OK

--

3 | Replace the remote control door lock receiver. Refer to Remote Control Door Lock Receiver Replacement . Is the replacement complete? | System OK | --