For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Power Door Locks System Check? | -- | Go to Step 2 | Go to Power Door Locks System Check
2 | Are both of the actuators inoperative? | -- | Go to Step 4 | Go to Step 3
3 | Is the left actuator inoperative? | -- | Go to Step 7 | Go to Step 16
4 | Test for a open using a J 39200 DMM in the BLU/BLK wire or in SP252. Does the circuit have an open? | -- | Go to Step 6 | Go to Step 5
5 | Replace the multifunction alarm module. Refer to Multifunction Alarm Module Replacement . Is the repair complete? | -- | Go to Power Door Locks System Check | --
6 | Repair the open in the BLU/BLK wire between the multifunction alarm module connector cavity 3 and the SP252. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Power Door Locks System Check | --
7 | Test the WHT/BLK wire using a J 39200 DMM and SP550/SP551for an open. Does the circuit have an open? | -- | Go to Step 8 | Go to Step 9
8 | Repair the open in the WHT/BLK wire between the LH door lock actuator and chassis G200. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Power Door Locks System Check | --
9 | Using a test lamp, probe the LH lock actuator connector cavity 6 to ground. Does the test lamp illuminate when you trigger the switch to UNLOCK? | -- | Go to Step 10 | Go to Step 11
10 | Using a test lamp, probe the LH lock actuator connector cavity 5 to ground. Does the test lamp illuminate when you trigger the switch to LOCK? | -- | Go to Step 13 | Go to Step 14
11 | Test the BLU/RED wire using a J 39200 DMM for an open. Does the wire have an open? | -- | Go to Step 12 | Go to Step 5
12 | Repair the open in the BLU/RED wire between the actuator connector and the alarm connector. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Power Door Locks System Check | --
13 | Replace the LH door lock actuator. Refer to Door Lock Switch Replacement . Is the repair complete? | -- | Go to Power Door Locks System Check | --
14 | Test the BLU/BLK wire and SP252 using a J 39200 DMM for an open. Does the circuit have an open? | -- | Go to Step 15 | Go to Step 5
15 | Repair the open in the BLU/BLK wire between the LH door lock actuator connector cavity 5 and the SP252. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Power Door Locks System Check | --
16 | Test the WHT/BLK wire, SP650, and SP250 using a J 39200 DMM for an open. Does the circuit have an open? | -- | Go to Step 17 | Go to Step 18
17 | Repair the open in the WHT/BLK wire between the RH front door lock actuator and chassis G200. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Power Door Locks System Check | --
18 | Using a test lamp, probe the RH lock actuator connector cavity 1 to ground. Does the test lamp illuminate when you trigger the switch to UNLOCK? | -- | Go to Step 19 | Go to Step 20
19 | Using a test lamp, probe the RH lock actuator connector cavity 2 to ground. Does the test lamp illuminate when you trigger the switch to LOCK? | -- | Go to Step 22 | Go to Step 23
20 | Test the GRN/WHT wire using a J 39200 DMM between the RH lock actuator and alarm module for an open. Does the wire have an open? | -- | Go to Step 21 | Go to Step 5
21 | Repair the open in the GRN/WHT wire between the RH front door lock actuator connector cavity 1 and the alarm connector. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Power Door Locks System Check | --
22 | Replace the RH front door lock actuator. Refer to Power Door Lock Actuator Replacement . Is the repair complete? | -- | Go to Power Door Locks System Check | --
23 | Test the BLU/BLK wire and SP252 using a J 39200 DMM for an open. Does the circuit have an open? | -- | Go to Step 24 | Go to Step 5
24 | Repair the open in the BLU/BLK wire between the RH front door lock actuator connector cavity 2 and SP252. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Power Door Locks System Check | --