For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
Schematic Reference: Radio/Audio System Schematics
1 | Did you review the Radio/Audio System Description and Operation and perform the necessary inspections? | Go to Step 2 | Go to Radio/Audio System Description and Operation
2 |

1. Turn ON the ignition, with the engine OFF.
2. Turn ON the radio.
3. Insert a cassette tape.

Does CLN appear in the radio display?

Go to Testing for Intermittent Conditions and Poor Connections in Wiring Systems

Go to Step 3

3 |

1. Clean the tape head path using the J 39916-A kit.
2. Reset the display by pushing and holding the eject button for 5 seconds.

Does the radio display flash three dashes and clear?

Go to Step 5

Go to Step 4

4 | Replace the radio. Refer to Radio Replacement . Did you complete the replacement? | Go to Step 5 | --
5 | Operate the system in order to verify the repair. Did you correct the condition? | System OK | Go to Step 3