For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel (IP) assembly. Refer to Instrument Panel Assembly Replacement in Instrument Panel, Gages and Console.
2. Remove the following components from the IP:

2.1. | The 4 screws

2.2. | The defroster outlet duct (1)

### Installation Procedure

1. Install the defroster outlet duct (1) to the IP. Secure the outlet duct with the 4 screws.
2. Install the IP assembly. Refer to Instrument Panel Assembly Replacement in Instrument Panel, Gages and Console.