For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Instrument Cluster System Check? | -- | Go to Step 2 | Go to Instrument Cluster System Check
2 |

1. Disconnect the instrument cluster assembly. Refer to Instrument Panel Assembly Replacement .
2. Using a J 39200 measure the resistance from the screw head IG+ to the screw head FU.

Is the measured resistance within the specified limits?

104-114 ohms

Go to Step 3

Go to Step 5

3 | Using a J 39200 measure the resistance from the screw head IG+ to the screw head SE. Is the measured resistance within the specified limits? | 221-231 ohms | Go to Step 4 | Go to Step 5
4 | Using a J 39200 measure the resistance from the screw head SE to the screw head FU. Is the measured resistance within the specified limits? | 114-124 ohms | Go to Step 6 | Go to Step 5
5 | Replace the fuel gauge. Refer to Fuel Gage Replacement . Is the repair complete? | -- | Go to Instrument Cluster System Check | --
6 | Inspect the instrument cluster printed circuit for damage or corrosion. Does the printed circuit have damage or corrosion? | -- | Go to Step 7 | Go to Step 8
7 | Replace the Printed circuit. Refer to Printed Instrument Cluster Circuit Replacement . Is the repair complete? | -- | Go to Instrument Cluster System Check | --
8 | Inspect the YEL/RED wire between the instrument cluster C3 and the fuel sender for damage or corrosion. Is the wire damaged? | -- | Go to Step 10 | Go to Step 9
9 | Inspect the BRN wire between the G202 and the fuel sender assembly for damage or corrosion. Is the wire damaged? | -- | Go to Step 10 | Go to Step 11
10 | Repair the wire. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Instrument Cluster System Check | --
11 | Replace the fuel sender assembly. Refer to Fuel Sender Assembly Replacement in Engine Controls. Is the repair complete? | -- | Go to Instrument Cluster System Check | --