For 1990-2009 cars

Important: Do not overheat the terminal when resoldering.

• | Reattach the rear defogger bus bar lead terminals by soldering. Use a solder containing 3 percent silver and a rosin flux paste.

• | Before soldering the bus bar lead terminal, buff the repair area using fine steel wool.

• | Apply the paste-type rosin flux in small quantities to the bus bar lead terminal repair area using a brush.

| Notice: Use only enough heat to melt the solder. Using excessive heat can damage the rear window defogger components or the rear window.

• | Coat the soldering iron tip using solder prior to the repair procedure. Use only enough solder in order to ensure a complete repair.