For 1990-2009 cars

Operation | Service Allowed | Service Preferred
--- | --- | ---
Front

- Caster (non adjustable, for reference only)

+0.57° to +2.07°

+1.32°

- Cross Caster (non adjustable, for reference only)

0.0° to +0.75°

0.0°

- Camber

-0.93° to +0.57°

-0.18°

- Cross Camber

0.0° to +0.75°

0.0°

- Toe

-0.05° to +0.15°

+0.05°

- Total Toe

-0.1° to +0.3°

+0.1°

- Inside Wheel Angle

37.22° to 41.22°

39.22°

- Outside Wheel Angle (reference)

--

33.37°

Rear

- Camber (non adjustable, for reference only)

-1.67° to -0.17°

-0.92°

- Cross Camber (non adjustable, for reference only)

0.0° to +0.75°

0.0°

- Toe

+0.1° to +0.3°

+0.2°

- Total Toe

+0.2° to +0.6°

+0.4°