For 1990-2009 cars

#### Steering and Suspension and Front Drive Axle Boot and Seal Inspection

Inspect the front and the rear suspension and the steering system for the following:

• | Damaged parts

• | Loose or missing parts

• | Signs of wear or lack of lubrication

Inspect the power steering lines and the hoses for the following:

• | Proper hookup

• | Binding

• | Leaks

• | Cracks

• | Chafing, etc.

Clean and then inspect the front wheel drive axle boot seals for damage, tears or leakage.

Service the vehicle as necessary.

#### Exhaust System Inspection

Inspect the complete system. Inspect the body near the exhaust system. Look for broken, damaged, missing or out-of-position parts as well as open seams, holes, loose connections or other conditions which could cause a heat build-up in the floor pan or could let exhaust fumes into the vehicle. Service the vehicle as necessary.

#### Engine Cooling System Inspection

Caution: NEVER spray water on a hot heat exchanger. The resulting steam could cause personal injury.

Notice: Compressed air or water can be used to clean the radiator fins. Do not exceed 138 kPa (20 psi). Pressure over 138 kPa (20 psi) will damage the radiator.

Inspect the hoses and replace if they are cracked, swollen or deteriorated.

Inspect all pipes, fittings and clamps; replace as needed.

Important: The radiator and A/C condenser should be kept clean for proper system performance. Cleaning is recommended at least once a year.

Inspect the front surface of the radiator and A/C condenser. Insects, leaves, debris, etc. can affect the performance of the radiator and A/C condenser.

If the front surface of either or both of these components is found to be in need of cleaning, the unwanted material can be removed by performing the following:

• | Ensure that the engine is off and cool.

• | Blow compressed air through the radiator from the rear surface of the radiator toward the front of the vehicle.

• | If compressed air is not available, use a water hose to force water through the radiator from the rear surface of the radiator toward the front of the vehicle.

To help ensure proper cooling system pressure performance, a pressure test of the cooling system and pressure cap is recommended at least once a year.

If their is a loss of coolant, refer to Loss of Coolant in Engine Cooling.

#### Throttle System Inspection

Throttle system (includes accelerator and cruise control) should operate freely without hesitation between full closed and wide open throttle.

Important: The accelerator and cruise control cables should not be lubricated under any condition. Throttle system components causing hesitation or sticking should be replaced.

Inspect the following:

• | Missing parts such as retainers or clips.

• | Interference of the linkage or the cable conduit to critical components such as fuel lines, brake lines, harness leads, etc.

• | Proximity of the cable to the exhaust system and other heat sources: check for melting and/or discoloration.

• | Cable kinking. Avoid sharp bends of cables.

• | Clearance of the throttle system moving parts throughout their travel from other stationary components.

• | Damage of the components due to cable kinking, severe kinking, severe abrasion, misalignment, etc. If any of the above conditions exists, notify your dealer for a recommended rerouting, adjustment, or replacement.

#### Brake System Inspection

Inspect the complete system.

Notice: A low brake fluid level can indicate worn disc brake pads which may need to be serviced. Also, if the brake system warning light stays on or comes on, something may be wrong with the brake system. If the anti-lock brake system warning light stays on or comes on, something may be wrong with the anti-lock brake system.

Inspect the brake lines and the hoses for the following:

• | Proper hookup

• | Binding

• | Leaks

• | Cracks

• | Chafing, etc.

Inspect the disc brake pads for wear. Inspect the rotors for surface condition. Inspect the drum brake linings for wear and cracks. Inspect other brake parts, including the drums, wheel cylinders, calipers, park brake, etc.

Check parking brake adjustment.

The brakes may need to be inspected more often if driving habits or conditions result in frequent braking.