For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel compartment. Refer to Instrument Panel Compartment Replacement in Instrument Panel, Gages and Console.
2. Disconnect the blower motor resistor electrical connector.
3. Remove the 2 screws and the blower motor resistor (4) from the blower case.

### Installation Procedure

1. Install the blower motor resistor (4) to the blower case. Secure with the 2 screws.
2. Connect the blower motor resistor electrical connector.
3. Install the IP compartment. Refer to Instrument Panel Compartment Replacement in Instrument Panel, Gages and Console.