For 1990-2009 cars

### Removal Procedure

1. Remove the inside door handle screw (1).
2. Slide the handle (2) forward and pull it away from the front side door trim (1).
3. Open the rod retainer (3) and remove the inside handle rod (4) from the inside door handle (2).
4. Remove the handle (2) from the vehicle.

### Installation Procedure

1. Install the inside handle rod (4) to the inside door handle (2). Secure the rod with the retainer (3).
2. Install the inside door handle (2) to the front door trim panel (3) and slide rearward. Secure the handle with the screw (1).