For 1990-2009 cars

### Removal Procedure

1. Remove the rear side door inside handle screw (1).
2. Slide the handle (2) forward and pull it away from the rear side door trim (3).
3. Remove the inside handle rod from the inside door handle (2).
4. Remove the handle (2) from the rear door trim panel (3).

### Installation Procedure

1. Install the inside handle rod to the inside door handle (2).
2. Install the inside door handle (2) to the rear door trim panel (3) and slide rearward. Secure the handle with the screw.