For 1990-2009 cars

### Removal Procedure

1. Remove the front bumper fascia. Refer to Front Bumper Fascia Replacement .
2. Remove the front bumper fascia energy absorber from the front bumper impact bar.
3. Remove the 4 nuts (2) which secure the front bumper impact bar.
4. Remove the front bumper impact bar (1) from the front bumper impact bar outer brackets.

### Installation Procedure

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Install the front bumper impact bar (1) to the front bumper impact bar outer brackets. Secure the impact bar with the 4 nuts (2).

Tighten
Tighten the front bumper impact bar nuts to 36 N·m (26 lb ft).

2. Install the front bumper fascia energy absorber from the front bumper impact bar.
3. Install the front bumper fascia. Refer to Front Bumper Fascia Replacement .