For 1990-2009 cars

Step | Action | Normal Result(s) | Abnormal Result(s)*
--- | --- | --- | ---
Vehicles not equipped with air conditioning have 1 fan motor. Vehicles equipped with air conditioning have 2 fan motors. For vehicles equipped with air conditioning refer to HVAC System Check in HVAC Systems with A/C-Manual.
1 | Start the engine and run until the engine coolant temperature reaches 93°C (199°F) |

• | The fan motor runs once the engine coolant temperature reaches 93°C (199°F).

• | The fan motor stops running when the engine coolant temperature drops below 83° C (181° F).

• | Cooling Fan Inoperative

• | Cooling Fan Always On - Auxiliary

* Refer to the appropriate symptom diagnostic table for the applicable abnormal result.